1. ls /pyboard
2. cp filename.py /pyboard //copy file to rshell esp32 micropython//
3. repl
4. import filename